|  |  |
| --- | --- |
| **Sand spreader**  With the Wille sand spreader, you can spread just the right amount of sand and ensure a smooth sand layer. The agitator shaft inside the tank prevents sand from hardening inside the tank and ensures smooth feeding of sand to the feeder drum. The spring-loaded thick rubber plate against the feeder drum ensures that only the desired amount of sand drips from the tank. A cradle guard prevents large stones and ice from dropping inside the sand spreader. The bearings are placed outside the tank, which makes it easier to service them and lengthens their service life. The sand spreader in the rear of Wille requires a rear lift or rear tilting device, allowing it to be filled by backing into a heap.   * The agitator shaft prevents malfunction in sand feeding * Flow control valve for adjusting the sand flow * The durable hot-galvanised tank has a long service life | **Posipač soli/rizle**  Sa Wille posipačem soli/rizle možete posipati pravu količinu soli/rizle. Osovina unutar posipača sprečava so da očvrsne unutar rezervoara i osigurava ravnomeran dovod soli. Debela gumena ploča sa oprugom na dobošu osigurava da samo željena količina soli izađe iz iz rezervoara. Rešetka sprečava da veliki komadi soli ili led upadnu unutar posipača. Ležajevi su postavljeni izvan rezervoara što olakšava njihovu zamenu i produžava životni vek. Posipač se kači pozadi na zadnju rampu za podizanje/naginjanje koja omogućava punjenje vožnjom unazad u gomilu.   * Osovina sprečava zgrušavanje soli * Ventil kontrolu protoka za podešavanje protoka soli * Izdržljiv pocinkovani rezervoar za dug radni vek |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Volume (liters)** | **Working width (mm)** | **Weight (kg)** | **Wille** |
| **Sand spreader 180** | 180 | 1100 | 215 | 265 |
| **Sand spreader 250** | 250 | 1100 | 210 | 365 |
| **Sand spreader 370** | 370 | 1400 | 275 | 465 |
| **Sand spreader 550 fixed** | 550 | 1700 | 330 | 665 |
| **Sand spreader 550 tipping** | 550 | 1700 | 425 | 665 |
| **Sand spreader 700 fixed** | 700 | 1950 | 530 | 865 |
| **Sand spreader 700 tipping** | 700 | 1950 | 625 | 865 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Zapremina (l)** | **Radna širina (mm)** | **Težina (kg)** | **Wille** |
| **Posipač soli/rizle 180** | 180 | 1100 | 215 | 265 |
| **Posipač soli/rizle 250** | 250 | 1100 | 210 | 365 |
| **Posipač soli/rizle 370** | 370 | 1400 | 275 | 465 |
| **Posipač soli/rizle 550 fiksni** | 550 | 1700 | 330 | 665 |
| **Posipač soli/rizle 550 obarajući** | 550 | 1700 | 425 | 665 |
| **Posipač soli/rizle 700 fiksni** | 700 | 1950 | 530 | 865 |
| **Posipač soli/rizle 700 obarajući** | 700 | 1950 | 625 | 865 |