|  |  |
| --- | --- |
| **De-icing Solution Spreader**  The solution spreader is used for spreading saline solution on streets, cycle paths and pavements, which allows you to keep them free of ice throughout the winter. The amount to be spread is automatically adjusted to the machine’s driving speed. You can choose the working width to be the central area of the spreader, or in addition the left or ride side, or both of them. The attachment is controlled from the display unit located in the cabin. Owing to the multi-hole nozzle, the saline solution does not spread as mist into the air. The baffle plates inside the tank prevent the solvent from splashing when travelling between locations.   * Working width adjustable between 2.5 to 5 m * Maximum flow by a single press of a button * The tank is filled through two stainless and easy-to-clean filters * The pump with a separate vacuum filter * Spreading ramp with a separate elevation adjustment * Supports for storing * A 15-metre hose reel for manual cleaning is available as an option * The machine must be equipped with electrical readiness for the solution spread | **Posipać za mokroposipanje**  Koristi se za posipanje tečnog rastvora po ulicama, biciklističkim stazama i trotoarima, što vam omogućava da ih održite da se ne zalede tokom zime.  Količina posipanja automatski se prilagođava brzini vožnje mašine. Možete odabrati da radna širina bude centralni deo posipača ili dodatno na levu ili desnu stranu ili na obe strane.  Posipačem se upravlja sa displeja koji se nalazi u kabini. Zahvaljujući mlaznicama sa više rupa, rastvor se ne raspršuje poput magle u vazduh. Pregradne ploče unutar rezervoara sprečavaju rastvor da se talasa tokom putovanja.   * Radna širina je podesiva od 2,5 d9 5 m. * Maksimalan protok jednim pritiskom na dugme * Rezervoar se puni kroz dva nerđajuća filtera koji se lako čiste * Pumpa sa odvojenim vakuum filterom * Rampa za prskanje sa zasebnim podešavanjem visine * Stope za odlaganje * Kolut sa metara creva za ručno čišćenje dostupan je kao opcija * Mašina mora biti opremljena električnim instalacijom za posipač |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Volume (liters)** | **Working width (mm)** | **Spread amount (g/m2)** | **Spreading speed (km/h)** | **Wille** |
| **De-icer 1500** | 1500 | 2500-5000 | 455 | max. 30 | 655,865 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Zapremina (l)** | **Radna širina (mm)** | **Količina posipanja (g/m2)** | **Brzina posipanja (km/h)** | **Wille** |
| **De-icer 1500** | 1500 | 2500-5000 | 455 | max. 30 | 655,865 |