|  |  |
| --- | --- |
| **Rotary brush**  Wille Optim rotary brush is just the right kind of work attachment for cleaning the ground of leaves, snow and sand. The brush is equipped with a sprinkler nozzle for dust suppression as standard equipment.   * For use all year round * The ends of the cylinder are free, making it possible to brush next to walls or kerbs * The lateral tilt of ± 6º makes it possible to achieve a good sweeping result * Hydraulic angle adjustment of ± 27° * Vertical floating movement of the cylinder of approximately 300 mm allows the cylinder to follow the elevations on the ground surface * Shock-dampers for smoother sweeping movement * Changing the lamella is easy; no need to demount the hydraulic motor | **Rotaciona četka**  Rotaciona četka je pravi izbor radnog priključka za čišćenje površina od lišća, senga i peska. Četka je opremljena mlaznicom za prskanje za suzbijanje prašine.   * Za upotrebu tokom cele godine * Krajevi četke su slobodni što omogućava čišćenje pored zidova i ivičnjaka * Poprečni nagib od ±6° omogućava postizanje dobrih rezultata čišćenja * Hidraulično podešavanje ugla od ±27° * Vertiklano plutajuće kretanje četke od oko 300mm omogućava četki da prati neravnine terena * Absorbcija udara osigurava ravnomerno četkanje * Zamena četke je jednostavna, ne potrebe za uklanjanje hidro-motora |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Min. Working width (mm)** | **Max. Working width (mm)** | **Weight (kg)** | **Wille** |
| **Rotary brush 140 \*)** | 1250 | 1400 | 320 | 265 |
| **Rotary brush 170** | 1515 | 1700 | 400 | 365 |
| **Rotary brush 200** | 1780 | 2000 | 450 | 465 |
| **Rotary brush 240** | 2040 | 2400 | 480 | 665, 865 |
| **Rotary brush 270** | 2400 | 2700 | 510 | 665, 865 |
| **Rotary brush 320** | 2850 | 3200 | 560 | 865 |

\*) Rotary brush 140 has a hydraulic horizontal movement to the left 220 mm and to the right 265 mm. The brush moves vertically 100 mm

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Min. Radna širina (mm)** | **Max. Radna širina (mm)** | **Težina (kg)** | **Wille** |
| **Rotaciona četka 140** | 1250 | 1400 | 320 | 265 |
| **Rotaciona četka 170** | 1515 | 1700 | 400 | 365 |
| **Rotaciona četka 200** | 1780 | 2000 | 450 | 465 |
| **Rotaciona četka 240** | 2040 | 2400 | 480 | 665, 865 |
| **Rotaciona četka 270** | 2400 | 2700 | 510 | 665, 865 |
| **Rotaciona četka 320** | 2850 | 3200 | 560 | 865 |

\*) Rotaciona četka 140 ima hidraulično horizontalno pomeranje u levo 220 mm i u desno 265 mm. Četka se pomera vertiklano 100 mm