|  |  |
| --- | --- |
| **Collecting sweeper**  With the collecting sweepers you can clean surfaces and collect the debris into a tank simultaneously. Dust suppression made easier by an integrated water tank which is equipped with sprinkler nozzles for the cup brush and the cylinder. As the tank and the brush move up and down along with the terrain, there is no need to separately lift and lower the device even at the speed bumps. The cup brush yields when it hits the walls or other obstacles. The bottom of the tank opens hydraulically for emptying, and owing to the Wille loader, you can empty the content e.g. to a lorry bed.   * Two work stages simultaneously – cleaning the surface and collecting the debris into the tank * The tank can be emptied, for example, onto a lorry bed * The tank floats in the vertical direction * Hydraulic opening of the bottom for emptying * Cup brush on the right-hand side as standard * Water tank on top of the unit, sprinkler nozzles for the cylinder and the cup brush * All models can be equipped with an extra cup brush * One support wheel in the front and two in the rea | **Čistilica sa spremnikom**  Pomoću čistilice sa spremnikom možete istovremeno čistiti površine i sakupljati prljavštinu u spremnik. Suzbijanje prašine radi se pomoću integrisanog rezervoara za vodu koji je opremljen prskalicama za bočnu i valjak četku. Obzirom da se rezervoar i četka kreću gore dole prateći teren, nema potrebe za dodatnim podizanjem i spuštanjem uređaja, čak ni kod ležećih policajaca. Bočna četka se savija prilikom udara u zidove ili druge prepreke. Dno spremnika se otvara hidraulično za pražnjenje, a zahvaljujući Wille prednjim utovarivačem, sadržaj možete isprazniti u kontejner.   * Dve faze rada istovremeno-čišćenje površine i sakupljanje prljavštine u spremnik. * Spremnik se može isprazniti u npr. Kontejner * Rezervoar se pomere u vertikalnom pravcu i prati nervnine terena * Hidraulično otvaranje dna za pražnjenje * Bočna četka sa desne strane kao deo standardne opreme * Rezervoar za vodu, prskalice za valjak i bočnu četku * Svi modeli mogu biti opremljeni sa dodatnom bočnom četkom * Jedan potporni točak napred i dva pozadi |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Volume (l)** | **Water tank volume (l)** | **Working width (mm)** | **Brush diameter (mm)** | **Weight (kg)** | **Wille** |
| **Collecting sweeper 205** | 200 | 100 | 1700, with extra cup brush 2050 | 600 | 525 | 365 |
| **Collecting sweeper 305** | 300 | 100 | 2050, with extra cup brush 2500 | 600 | 560 | 465 |
| **Collecting sweeper 650** | 560 | 200 | 2250, with extra cup brush 2700 | 700 | 790 | 665, 865 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Zapremina spreminka (l)** | **Zapremina rezervoara za vodu (l)** | **Radna širina (mm)** | **Prečnik četke (mm)** | **Težina (kg)** | **Wille** |
| **Čistilica sa spremnikom 205** | 200 | 100 | 1700, sa bočnom četkom 2050 | 600 | 525 | 365 |
| **Čistilica sa spremnikom 305** | 300 | 100 | 2050, sa bočnom četkom 2500 | 600 | 560 | 465 |
| **Čistilica sa spremnikom 650** | 560 | 200 | 2250, sa bočnom četkom 2700 | 700 | 790 | 665, 865 |