|  |  |
| --- | --- |
| **High-pressure washer**  Wille Optim high-pressure washers are ideal for removal of fine-grained dirt and dust from the asphalt. For a smoother washing result, the washer directs water evenly to each nozzle. You can turn the nozzle pipe and decide the direction in which the dirt is to be removed. With the help of a hose reel, you can clean places that are hard to access, such as gateways, etc. The baffle plates inside the tank make the motion smoother when travelling between locations. In connection with the collecting sweeper you can use the washer tank water for dust suppression.   * The refill water is filtered by three stainless, easy-to-clean filters. * The nozzle pipe can be turned hydraulically * A 15-metre hose reel for manual cleaning is available as an option * Support legs for storing | **Pranje pod visokim pritiskom**  Wille Optim priključak za pranje pod visokim pritiskom idealan je za uklanjanje sitnozrne prljavštine i prašine iz asfalta. Za bolji rezultat pranja, voda se ravnomerno usmerava u svaku mlaznicu. Možete okrenuti cev sa mlaznicama i odabrati u kom pravcu ćete uklanjati prljavštinu. Pomoću creva i puške za ručno pranje možete očisiti teško pristupačna mesta. Pregradne ploče unutar rezervoara sprečavaju talasanje vode prilikom transporta između lokacija. U kombinaciji sa čistilicom za skupljanje prljavštine, možete koritstiti rezervoar za vodu za uklanjanje prašine prilikom čišćenja.   * Voda koja se doliva filtrira se putem tri nerđajuća filtera, koji se lako čiste * Cev sa mlaznicama se može hidraulično okretati * Kolut sa 15 metara creva za ručno čišćenje dostupan je kao opcija * Stope za odlaganje |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Volume (liters)** | **Max. Pressure (bar)** | **Max pump flow (l/min)** | **Weight (kg)** | **Wille** |
| **High-pressure washer 550** | 550 | 130 | 30 | 230 | 265, 365 |
| **High-pressure washer 1000** | 1000 | 150 | 45 | 435 | 455B, 465 |
| **High-pressure washer 1500** | 1500 | 150 | 90 | 635 | 665,865 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Zapremina (l)** | **Max. Pritisake (bar)** | **Max protok pumpe (l/min)** | **Težina (kg)** | **Wille** |
| **High-pressure washer 550** | 550 | 130 | 30 | 230 | 265, 365 |
| **High-pressure washer 1000** | 1000 | 150 | 45 | 435 | 455B, 465 |
| **High-pressure washer 1500** | 1500 | 150 | 90 | 635 | 665,865 |