|  |  |
| --- | --- |
| **Mulcher**  Mulcher with side adjustment is purposed to keep sidewalks and road sides clean. With this very quiet attachment you can mulch alongside paths and roads, as well as slopes and ditches.   * Hydraulic side adjustment of 104 cm * Mulching of grass and light wood * Inclination range: upward 90 ˚, downward 60 ˚ | **Tarup**  Tarup sa bočnim pomeranjem predviđen je za održavanje povrišna pored puta i trotoara. Ovim veoma tihim piključkom možete kositi pored staza i puteva kao i nasipa i jarka.   * Hidraulično bočno pomeranje od 104 cm * Košenje trave i lakog drveća * Mogućnost nagiba: na gore 90°, na dole 60° |