|  |  |
| --- | --- |
| **High-tipping bucket**  When the lifting height of the standard bucket is not enough, the answer is a high-tipping bucket. It gives you a notably higher lifting height for loading snow, for example.   * For loading light materials * Notably higher dumping height and distance in comparison with the standard bucket | **Visoko utovarna kašika**  Kada visina podizanja standardne kašika nije dovoljna, odgovor je visokoutovarna kašika. Ona vam pruža znatno ceću visinu podizanja za utovar.   * Za utovar lakih materijala * Znatno veća visina istovara i udaljenost u odnosu na standardnu kašiku |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Volume (liters)** | **Working width (mm)** | **Emptying height (mm)** | **Weight (kg)** | **Wille** |
| **HT-bucket 550** | 550 | 1580 | 1000 (265)  3130 (365) | 300 | 265, 365 |
| **HT-bucket 800** | 800 | 2700 | 3400 | 400 | 465 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Zapremina (l)** | **Radna širina (mm)** | **Visina istovara (mm)** | **Težina (kg)** | **Wille** |
| **Visoko utovarna kašika 550** | 550 | 1580 | 1000 (265)  3130 (365) | 300 | 265, 365 |
| **Visoko utovarna kašika 800** | 800 | 2700 | 3400 | 400 | 465 |