|  |  |
| --- | --- |
| **Access platform Wille 9**  The access platform, specially designed for Wille, makes it possible to carry out a variety of maintenance work.  All the movements can be operated safely from the platform, so there is no need for another driver. The unit is equipped with hydraulic support outrigg. It is approved for use with Wille 365 - 865 models. The attachment is connected to the rear lift of the base machine. | **Hidraulična platforma sa korpom za rad na visini – Wille 9**  Hidraulična platforma za rad na visini, posebno dizajnirana za Wille, omogućava obavljanje različitih poslova održavanja.  Svim pokretima se može bezbedno upravljati sa platforme, tako da nema potrebe za drugim vozačem. Platforma je opremljena sa hidrauličnim potpornim stopama. Odobrena je za upotrebu za modele Wille 365 – 865. Priključak se kači na uređaj za kačenje koji se nalazi u zanjem delu osnovne mašine. |

|  |  |
| --- | --- |
| **Wille 9 Access platform** | |
| Working height (mm) | 8800 |
| Platform floor from the ground (mm) | 6800 |
| Outreach to the side (mm) | 5700 |
| Swing angle of the boom (degrees) | ± 70° |
| Platform load (kg) | 120 (1 person + 40) |
| Platform dimensions (mm) | 820 x 740 |
| Weight (kg) | 720 |
| Compatibility | 365, 465, 665, 865 \* |

\*) Attachment compatibility requires separately sold optional features in the base machine.

|  |  |
| --- | --- |
| **Hidraulična platforma sa korpom za rad na visini Wille 9** | |
| Radna visina (mm) | 8800 |
| Pod platforme od tla (mm) | 6800 |
| Bočni doseg (mm) | 5700 |
| Ugao zakretanja strele (stepeni) | ± 70° |
| Nosivost (kg) | 120 (1 osoba + 40) |
| Dimenzije platforme (mm) | 820 x 740 |
| Težina (kg) | 720 |
| Kompatibilnost | 365, 465, 665, 865 \* |

\*) Da bi priključak bio kompatibilan to zahteva određene funkcije u osnovnoj mašini koje su opcione.