|  |  |
| --- | --- |
| **Leaf bucket**  Leaf buckets are used for collecting light leaves and twigs. Can be used as snow bucket without the hatch. One work attachment, multiple uses.  The bucket is equipped with a manually opening top hatch, where from the collected material can be put inside the bucket without that the material would, for example, be exposed to gusts of wind for the whole width of the bucket.  The whole cover can be opened and closed hydraulically from the cabin of the machine. | **Kašika za lišće**  Kašika za lišće se koristi za sakupljanje lišća i grančica. Može se koristiti kao kašika za sneg ili kao utovarna kašika bez poklopca. Jedan radni priključak, višestruka upotreba.  Kašika je opremljena ručnim otvorom gornjeg poklopca, gde se sakupljeni materijal može ubaciti unutar kašike bez da materijal bude izložen naletima vetra.  Čitav poklopac se može hidraulično otvarati i zatvarati iz kabine mašine. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Volume (liters)** | **Working width (mm)** | **Weight (kg)** | **Wille** |
| **Leaf bucket 1200** | 1200 | 1950 | 455 | 465 |
| **Leaf bucket 1900** | 1900 | 2300 | 615 | 655, 865 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Zapremina (l)** | **Radna širina (mm)** | **Težina (kg)** | **Wille** |
| **Kašika za lišće 1200** | 1200 | 1950 | 455 | 465 |
| **Kašika za lišće 1900** | 1900 | 2300 | 615 | 655, 865 |