|  |  |
| --- | --- |
| **Multi-functional bucket**  The multi-function bucket is designed for collecting and loading snow from yards and parking areas Owing to the wings, it can also be used for plowing To collect snow, you can use the wings to widen the plowing width by one third or choose to use only one of them. Spring-loaded blades guarantee that the attachment does not start to steer the machine, but rather makes it adjust to the movements of the machine and the shape of the ground surface. The swing cylinders in wings are equipped with safety valves which prevent damage should the bucket bang against an obstacle. For the wearing surface, in addition to a straight-edged blade, a punched blade is available, which leaves the ground less slippery and slightly more rough after snow plowing.   * Optionally available with straight-edged or punched blade * Wings equipped with spring-loaded blades * Swing cylinders equipped with safety valves which prevent damage in collisions | **Multifunkcionalna kašika**  Multifunkcionalna kašika dizajnirana je za sakupljanje i utovar snega iz dvorišta i parkirališta. Zahvaljujući bočnim stranicama može se koristiti i kao raonik. Kada sakupljate sneg možete proširiti kašiku bočim stranicama da povećate površinu pluga za jednu trećinu ili možete odlučiti da otvorite samo jednu stranicu. Noževi sa oprugom obezbeđuju da priključak ne počne da upravlja mašinom, već da prati pokrete mašine i površinu tla.  Cilindri na bočnim stranicama opremljeni su sigurnosnim ventilima koji sprečavaju oštećenje u slučaju da kašika naleti na prepreku. Pored ravnog noža na raspolaganju je i mrežasto sečivo koje čini tlo hrapavijim i manje klizavim.   * Opciono dostupna sa ravnim nožem ili sa mrežastim * Bočne stranice opremljene noževima sa oprugama * Cilindri na bočnim strnicama opremljeni sigurnosnim ventilima koji sprečavaju oštećenja u slučaju udara u prepreku |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Volume (l)** | **Min. Working width (mm)** | **Max. Working width (mm)** | **Weight (kg)** | **Wille** |
| **Multi-functional Bucket 750** | 750 | 1720 | 2685 | 290 | 365 |
| **Multi-functional Bucket 1000** | 1000 | 1825 | 3000 | 385 | 465 |
| **Multi-functional Bucket 1500** | 1500 | 2100 | 3590 | 575 | 665 |
| **Multi-functional Bucket 2000** | 2000 | 2500 | 4000 | 685 | 865 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Zapremina (l)** | **Min. Radna širina (mm)** | **Max. Radna širina (mm)** | **Težina (kg)** | **Wille** |
| **Multifunkcionalna kašika 750** | 750 | 1720 | 2685 | 290 | 365 |
| **Multifunkcionalna kašika 1000** | 1000 | 1825 | 3000 | 385 | 465 |
| **Multifunkcionalna kašika 1500** | 1500 | 2100 | 3590 | 575 | 665 |
| **Multifunkcionalna kašika 2000** | 2000 | 2500 | 4000 | 685 | 865 |